For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement .
2. Remove the rear compartment spare tire cover.
3. Remove the cargo net. Refer to Cargo Net Replacement .
4. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
5. Remove the rear seat back. Refer to Rear Seat Back Replacement in Seats.
6. Remove the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.

Important: The rear compartment trim panel is a two-piece molded unit.

7. Fold the right section of the rear compartment trim panel toward the center of the compartment.
8. Fold the left section of the rear compartment trim panel toward the center of the compartment.
9. Remove the trim panels from the rear compartment.

### Installation Procedure

1. Position the folded trim panels into the rear compartment, with the topmost panel on the left.
2. Install the trim panels over the seat brackets and press the trim panels up under the quarter panels.
3. Install the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.
4. Install the rear seat back. Refer to Rear Seat Back Replacement in Seats.
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
6. Install the cargo net. Refer to Cargo Net Replacement .
7. Install the rear compartment spare tire cover.
8. Install the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement .