For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front wheel and tire. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Disconnect the backup lamp switch harness connector.
4. Remove the backup lamp switch from the transaxle.

### Installation Procedure

1. Install the backup lamp switch to the transaxle.
2. Connect the backup lamp switch harness connector.
3. Install the front left wheel and tire. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Lower the vehicle.