For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cylinder Valve End Fitting | 27 N·m | 20 lb ft
Cooler Pipe Bracket Bolts | 10 N·m | 89 lb in
Inner Tie Rod End | 100 N·m | 74 lb ft
Intermediate Shaft Lower Pinch Bolt | 17 N·m | 13 lb ft
Power Steering Gear Bolts | 110 N·m | 81 lb ft
Power Steering Hose Retaining Nut W/L61 | 5 N·m | 45 lb in
Power Steering Pressure Hose Fitting | 27 N·m | 20 lb ft
Power Steering Pump Flow Control Valve | 75 N·m | 55 lb ft
Power Steering Pump Mounting Bolts W/LA1 | 34 N·m | 25 lb ft
Power Steering Mounting Bolts W/L61 | 26 N·m | 19 lb ft
Power Steering Return Hose Fitting | 27 N·m | 20 lb ft
Power Steering Return Hose Support Nut | 50 N·m | 37 lb in
Power Steering Return Pipe Fitting | 27 N·m | 20 lb ft
Tie Rod Jam Nut | 75 N·m | 16 lb ft
Tie Rod Nut

- First Pass

20 N·m

15 lb ft

- Final Pass

+ 180°

Valve End Fitting | 27 N·m | 20 lb ft