For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the front tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the stabilizer shaft. Refer to Stabilizer Shaft Replacement .
4. Remove the stabilizer shaft bushings (1) from the stabilizer shaft (2).

### Installation Procedure

1. Install the stabilizer shaft bushings (1) to the stabilizer shaft (2).
2. Install the stabilizer shaft. Refer to Stabilizer Shaft Replacement .
3. Install the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Lower the vehicle.