For 1990-2009 cars

Replace the wheels if the following conditions exist:

• | Bends

• | Dents

• | Excessive lateral or radial runout

• | Air leaks through the welds

• | Elongated bolt holes

• | The wheel nuts will not stay tight.

• | Excessive rust

Wheels with excessive runout may cause objectionable vibrations.

Replacement wheels must be equivalent to the original equipment wheels in the following areas:

• | Load capacity

• | Diameter

• | Rim width

• | Offset

• | Mounting configuration

A wheel of improper size or type may affect the following conditions:

• | Wheel and bearing life

• | Brake cooling

• | Speedometer/odometer calibration

• | Vehicle ground clearance

• | Tire clearance to the body and chassis

Steel wheels can be identified by a two or three-letter code stamped into the rim near the valve stem. Aluminum wheels have the code, part number, and manufacturer ID cast into the back of the wheel.