For 1990-2009 cars

The Data Display function contains lists of ABS and ETS data parameters. A brief description of all ABS and ETS data parameters available on the scan tool are listed below. The list is arranged in alphabetical order.

ABS Active: The scan tool displays Yes or No - The scan tool displays Yes when the ABS is active. This scan tool displays No during normal vehicle operation.
ABS Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the ABS indicator ON.
ABS Equipped: The scan tool displays Yes or No - The scan tool displays if vehicle is equipped with ABS.
ABS Relay Command: The scan tool displays On or Off - The scan tool displays On during vehicle operation. The EBCM commands the ABS relay On when Ignition positive voltage is present.
ABS Relay Feedback: The scan tool displays On or Off - The scan tool displays On during vehicle operation.
ABS Warning Lamp: The scan tool displays Off or On Indicates if the EBCM is commanding the ABS indicator ON.
Auto Learn Mode Active: The scan tool displays Yes or No. Indicates if TIM is currently in learn mode.
Battery Voltage: The scan tool displays 0 to 30 volts. The voltage measured between the module's battery positive voltage circuit and ground circuit.
BFC Option Config. No.: The scan tool displays 4 characters - The scan tool displays the BFC Option Configuration Number of the BCM.
Brake Fluid Level: The scan tool displays Low or Normal - The scan tool displays if the brake fluid level is below the standard operating level.
Brake Switch Status: The scan tool displays Applied or Released - The scan tool displays the state of the brake switch.
Calibration ID: The scan tool displays the 4 digit calibration ID of the control module.
Configuration ID: The scan tool displays 6 characters - The scan tool displays the configuration ID number of the EBCM.
DE Base Part Number: The scan tool displays 4 characters - The scan tool displays the base part number of the EBCM.
DE Build Sequence Number: The scan tool displays 8 characters - The scan tool displays the build sequence number of the EBCM.
DE Calibration Part Number: The scan tool displays 4 characters - The scan tool displays the calibration number of the EBCM.
DE End Model Part Number: The scan tool displays 4 characters - The scan tool displays the end model part number of the EBCM.
DE ROM Part Number: The scan tool displays 4 characters - The scan tool displays the ROM part number of the EBCM.
DRP Equipped: The scan tool displays Yes or No - The scan tool displays if vehicle is equipped with DRP.
EBCM to PCM Requested: The scan tool displays 0-100 percent - The scan tool displays the torque signal. The signal is used to transmit how much torque the EBCM is requesting the PCM to deliver. Normal values are between 10 and 100 percent. The signal should be at 100 percent when ETS is not active and at lower values when ETS is active.
ETS Active: The scan tool displays Yes or No - The scan tool displays whether or not the vehicle is currently in an ETS event.
ETS Active Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the LOW TRAC indicator ON.
ETS Disable Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the TRAC OFF indicator ON.
ETS Equipped: The scan tool displays Yes or No - The scan tool displays if vehicle is equipped with ETS.
ETS Status: The scan tool displays Off or On - The scan tool displays the state of the ETS based on if the driver has disabled ETS by pressing the ETS switch, or if the ETS has been disabled due to a malfunction.
ETS Warning Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the TRAC OFF indicator ON.
Ignition 0: The scan tool displays 0-17 volts - The scan tool displays the level of ignition positive voltage at the IPC.
Ignition Voltage: The scan tool displays 0-17 volts - The scan tool displays the level of ignition positive voltage at the EBCM.
Julian Date Code: The scan tool displays year/day - The scan tool displays the last digit of the year and the day of the year that the EBCM was built.
Left Front Wheel Speed: The scan tool displays 0-255 km/h (0-158 mph) - The scan tool displays the actual speed of the left front wheel.
Left Rear Wheel Speed: The scan tool displays 0-255 km/h (0-158 mph) - The scan tool displays the actual speed of the left rear wheel.
LF Inlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the LF inlet solenoid valve.
LF Outlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the LF outlet solenoid valve.
Low Tire Pressure: The scan tool displays Yes or No. Indicates if the EBCM has determined that a tire has low pressure.
Low Tire Press. Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the low tire pressure indicator ON.
Low Traction Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the LOW TRAC Indicator ON.
LR Inlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the LR inlet solenoid valve.
LR Outlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the LR outlet solenoid valve.
Monitor Mode 1: The scan tool displays Yes or No. Indicates if TIM is currently in mode 1 monitoring. The EBCM has limited detection capability for a low tire condition and has only partially learned the tire inflation configuration for the speed range.
Monitor Mode 2: The scan tool displays Yes or No. Indicates if TIM is currently in mode 2 monitoring. The EBCM has full detection capability for a low tire condition and has fully learned the tire inflation configuration for the speed range.
PCM to EBCM Delivered: The scan tool displays 0-100 percent - The scan tool displays the Requested Torque signal. The signal is used to transmit how much engine torque the PCM is delivering. Normal values are between 10 and 100 percent. The signal is at low values at idle and at higher values under driving conditions.
Pump Motor Commanded State: The scan tool displays On or Off - The scan tool displays the commanded state of the pump motor.
Pump Motor Feedback State: The scan tool displays On or Off - The scan tool displays the actual state of the pump motor.
Right Front Wheel Speed: The scan tool displays 0-255 km/h (0-158 mph) - The scan tool displays the actual speed of the right front wheel.
Right Rear Wheel Speed: The scan tool displays 0-255 km/h (0-158 mph) - The scan tool displays the actual speed of the right rear wheel.
RF Inlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the RF inlet solenoid valve.
RF Outlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the RF outlet solenoid valve.
Rough Road Parameter: The scan tool displays 0-1g - The scan tool displays the EBCM calculation of the road surface roughness. This information is sent to the PCM over the class 2 serial data line. The PCM uses this information for misfire detection.
RR Inlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the RR inlet solenoid valve.
RR Outlet Valve Solenoid: The scan tool displays Active or Inactive - The scan tool displays the commanded state of the RR outlet solenoid valve.
Software Version: The scan tool displays the software version of the IPC.
Steering Position Sensor: Displays 0 to 5 volts. The analog steering wheel position sensor signal, roughly 2.5 volts means that the steering wheel is centered.
Switched Battery Voltage: The scan tool displays 0-17 volts - The scan tool displays the level of the internal EBCM switched battery voltage available to the solenoid valves and pump motor.
System ID: The scan tool displays the configuration ID of the EBCM.
TIM Equipped: The scan tool displays Yes or No - The scan tool displays if vehicle is equipped with TIM.
TIM Reset Switch: The scan tool displays Was Pressed. Indicates if the TIM reset switch was pressed.
TIM System Enabled: The scan tool displays Yes or No - The scan tool displays if the TIM system is enabled as an option.
Torque Delivered Signal: The scan tool displays 0 to 100%. The duty cycle of the delivered torque signal. The duty cycle of the signal is used to transmit how much engine torque the PCM is delivering. Normal values are between 10 and 90 percent duty cycle. The signal is at low values (approximately 10 percent) at idle and at higher values under driving conditions.
Torque Request Signal: The scan tool displays 0 to 100%. The duty cycle of the requested torque signal. The duty cycle of the signal is used to transmit how much engine torque the EBCM is requesting the PCM to deliver. Normal values are between 10 and 90 percent duty cycle. The signal is at 90 percent duty cycle when traction control is not active and at lower values (approximately 10 percent) when traction control is active.
Traction Control: The scan tool displays Active or Inactive. The active status of the TCS. Indicates if TCS is currently active.
Traction Control Status: The scan tool displays Active or Inactive. The active status of the TCS. Indicates if TCS is currently active.
Traction Off Lamp: The scan tool displays Off or On. Indicates if the EBCM is commanding the TRAC OFF indicator ON.
Traction Switch: Display Off or On. Indicates the status of the traction control switch.
Vehicle Speed: The scan tool displays 0-255 km/h (0-158 mph) - This parameter displays the vehicle speed. The Powertrain Control Module (PCM) receives reference pulses from the Vehicle Speed Sensor (VSS) and converts them into km/h or MPH for display.
VES Actuator Commanded: Displays -3.3 to 3.3 amps. The amount of current that the EBCM is commanding to the variable effort steering actuator.
VES Actuator Feedback: Displays -3.3 to 3.3 amps. The actual amount of current that the variable effort steering actuator is drawing from the EBCM. The scan tool display the absolute value (i.e. positive value) of the feedback current.
VES Equipped: The scan tool displays Yes or No - The scan tool displays if vehicle is equipped with VES.