For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform a Diagnostic System Check for the Doors system? | Go to Step 2 | Go to Diagnostic System Check - Power Door Systems
2 | Verify that the rear power window lockout function is inoperative. Does the rear power window lockout function operate properly? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Replace the Driver Power Window Switch. Refer to Front Side Door Window Switch Replacement . Did you complete the repair? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2