For 1990-2009 cars

### Circuit Description

The intake air temperature (IAT) sensor is a thermistor which measures the temperature of the air entering the engine. The powertrain control module (PCM) applies 5 volts through a pull-up resistor to the IAT sensor. When the intake air is cold, the sensor resistance is high and the PCM will monitor a high signal voltage on the IAT signal circuit. If the intake air is warm, the sensor resistance is lower causing the PCM to monitor a lower voltage. DTC P1112 will set when the PCM detects an intermittently low signal voltage on the intake air temperature sensor signal circuit.

### Conditions for Running the DTC

• | DTCs P0101, P0102, P0103, P0117, P0118, P0125, P0128, P0502, P0503, P1114, or P1115 are not set.

• | The engine has been running for over 10 seconds.

• | The vehicle speed is more than 40 km/h (25 mph).

### Conditions for Setting the DTC

• | The IAT sensor indicates an intake air temperature intermittently more than 135°C (275°F).

• | The conditions are present for up to 5 seconds.

### Action Taken When the DTC Sets

• | The control module stores the DTC information into memory when the diagnostic runs and fails.

• | The malfunction indicator lamp (MIL) will not illuminate.

• | The control module records the operating conditions at the time the diagnostic fails. The control module stores this information in the Failure Records.

• | The driver information center, if equipped, may display a message.

### Conditions for Clearing the DTC

• | A current DTC Last Test Failed clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other non-emission related diagnostic.

• | Clear the DTC with a scan tool.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | With a scan tool, select diagnostic trouble codes (DTC). Does the scan tool indicate DTC P0112 also set? | Go to DTC P0112 | Go to Step 3
3 | Test the signal circuit for an intermittent short to ground. Refer to Testing for Intermittent Conditions and Poor Connections and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 4 | Go to Intermittent Conditions
4 |

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Failure Records conditions as noted.

Does the DTC reset?

Go to Step 2

System OK