For 1990-2009 cars

### Removal Procedure

The knuckle is a machined aluminum casting. Do not use a hammer in order to loosen suspension components attached to the knuckle. Do not pry or hammer on the aluminum knuckle in any way. Following these instructions will avoid damage to parts and systems.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Scribe the strut to the knuckle. Refer to Strut and Knuckle Scribing in Front Suspension.
4. Remove the strut mount to body nut (1) in the trunk area.
5. Remove the strut bolts (3) from inside the fender well.
6. Remove the strut knuckle bolts (5) and nuts (3) from the strut (1).
7. Remove the strut (1) from the vehicle.

### Installation Procedure

1. Loosely install the strut to knuckle bolts (5) and nuts (3).

Important: Align the scribe marks in order to ensure proper alignment.

2. Install the strut to body bolts (3) inside the fender well.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the strut mount to body nuts (1) in the trunk area.

Tighten

• | Tighten the nuts to 25 N·m (18 lb ft).

• | Tighten thestrut to knuckle bolts to 120 N·m (89 lb ft).

4. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
5. Lower the vehicle.
6. Check the wheel alignment. Refer to Wheel Alignment Measurement in Wheel Alignment.