For 1990-2009 cars

Table 1: | Forward - Back Motor
Table 2: | Height Motor, Front
Table 3: | Height Motor, Rear
Table 4: | Power Seat Switch (AG1 Only)
Table 5: | Power Seat Switch (AH3 Only)

#### Forward - Back Motor

Connector Part Information |

• | 12092110

• | 2-Way F Metri-Pack 480 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 285 | Power Seat Motor Feed-Driver (Horizontal Fore)
B | LT GRN | 284 | Power Seat Motor Feed-Driver (Horizontal Aft)

#### Height Motor, Front

Connector Part Information |

• | 12020556

• | 2-Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 287 | Power Seat Motor Feed-Driver (Front Vertical Down)
B | DK GRN | 286 | Power Seat Motor Feed-Driver (Front Vertical Up)

#### Height Motor, Rear

Connector Part Information |

• | 12052109

• | 2-Way F Metri-Pack 480 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 283 | Power Seat Motor Feed-Driver (Rear Vertical Down)
B | YEL | 282 | Power Seat Motor Feed-Driver (Rear Vertical Up)

#### Power Seat Switch (AG1 Only)

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 540 | Fuse Output, Battery
B | PNK | 282 | Power Seat Motor Feed-Driver (Rear Vertical Up)
C | PPL | 283 | Power Seat Motor Feed-Driver (Rear Vertical Down)
D | BLK | 550 | Ground
E | GRY | 286 | Power Seat Motor Feed-Driver (Front Vertical Up)
F | WHT | 287 | Power Seat Motor Feed-Driver (Front Vertical Down)
G | LT GRN | 284 | Power Seat Motor Feed-Driver (Horizontal Aft)
H | TAN | 285 | Power Seat Motor Feed-Driver (Horizontal Fore)

#### Power Seat Switch (AH3 Only)

Connector Part Information |

• | 12052854

• | 7-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 550 | Ground
B | DK GRN | 286 | Power Seat Motor Feed-Driver (Front Vertical Down)
C | DK BLU | 287 | Power Seat Motor Feed-Driver (Front Vertical Up)
D-E | -- | -- | Not Used
F | ORN | 540 | Fuse Output, Battery
G | BLK | 550 | Ground