For 1990-2009 cars

# Info - Using Caution When Servicing Final Drive Unit on 4T65-E Transaxles to Insure Thrust Bearing (695) is Properly Seated/Located

Subject: | Using Caution When Servicing Final Drive Unit on 4T65-E Transaxles To Insure Internal Gear Thrust Bearing (695) is Properly Seated/Located

Models: | 2001-2005 GM Passenger Cars

| with 4T65-E Transaxle (RPO's MN3, MN7, M15 or M76)

When servicing a final drive unit on a 4T65-E transaxle, use extreme caution to ensure that the internal gear thrust bearing (695) is properly seated/located.

It has been found that after servicing a final drive unit on 4T65-E transaxles, the internal gear thrust bearing (695) was not properly seated/located causing internal damage and a repeat repair.

Use a generous amount of Transgel J 36850 when installing the internal gear thrust bearing (695) to the park gear (696) to ensure the internal thrust bearing (695) will retain its proper position during assembly.