For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the stabilizer shaft. Refer to Stabilizer Shaft Replacement .
3. Remove the insulator (4) from the stabilizer shaft (2).

### Installation Procedure

1. Install the insulator (4) to the stabilizer shaft (2).
2. Install the stabilizer shaft to the vehicle. Refer to Stabilizer Shaft Replacement .
3. Lower the vehicle.