For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Clynder Valve End Fitting | 17 N·m | 13 lb ft
Inner Tie Rod End | 100 N·m | 74 lb ft
Intermediate Shaft Lower Pinch Bolt | 20 N·m | 15 lb ft
Power Steering Hose Retainer Nut | 50 N·m | 11 lb in
Power Steering Pressure Hose Fitting | 27 N·m | 20 lb ft
Power Steering Pump Mounting Bolts | 34 N·m | 25 lb ft
Power Steering Return Hose Fitting | 27 N·m | 20 lb ft
Power Steering Return Hose Support Nut | 50 N·m | 37 lb in
Power Steering Return Pipe Fitting | 27 N·m | 20 lb ft
Steering Gear Bolts | 110 N·m | 81 lb ft
Tie Rod Jam Nut | 75 N·m | 55 lb ft
Tie Rod Nut | 20 N·m plus 180 degrees rotation | 15 lb ft plus 180 degrees rotation