For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to disengage the clips located at the front and rear of the switch.
2. Rotate the switch down and to the left to remove it.
3. Disconnect the connector from the sunroof control switch.
4. Remove the sunroof control switch from the vehicle.

### Installation Procedure

1. Connect the connector (2) to the sunroof control switch (1).
2. Rotate the sunroof control switch into the headliner and press to engage the clips.