For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Audible Warnings Schematics DEFINITION: One or more chime functions are inoperative.
1 | Did you perform the Audible Warnings Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Audible Warnings
2 |

1. Install a scan tool.
2. Turn the ignition ON, with the engine OFF.
3. With a scan tool, perform the Chime Tone Test in the Radio.

Does the chime sound?

Go to Step 3

Go to Step 4

3 |

1. Turn OFF the ignition.
2. Open the driver's door.

Do the courtesy lamps illuminate when the driver's door is opened?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Courtesy Lamps Inoperative in Lighting Systems

4 |

1. Turn the radio ON.
2. Adjust the radio balance and fade to the left front speaker.

Does the speaker operate properly?

Go to Step 5

Go to Speakers Inoperative - One or More in Entertainment

5 | Important: Perform the set up procedure for the replacement radio. Replace the radio. Refer to Radio Replacement in Entertainment. Did you complete the replacement? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2