For 1990-2009 cars

### Removal Procedure

1. Remove the door handle bezel. Refer to Door Handle Bezel Replacement .
2. Remove the bolt (2) which secures the inside handle.
3. Remove the inside handle rod (4).
4. Remove the door lock rod (2).
5. Remove the inside door handle (3).

### Installation Procedure

1. Install the inside door handle (3).
2. Install the door lock rod (2).
3. Install the inside handle rod (4).
4. Install the inside handle bolt (2).
5. Install the inside handle bezel. Refer to Door Handle Bezel Replacement .