For 1990-2009 cars

### Diagnostic Aids

Inspect the clutch pedal for a loose or worn clutch pedal spring. If the clutch pedal stays to the floor you should check the master cylinder for improper fluid level or faulty parts. Also inspect the hydraulic hoses or pipes for damage or even leaks. Inspect the clutch diaphragm springs to see if they are broken.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step inspects for the correct fluid level in the reservoir.

3. This step inspects the hydraulic lines for kinks, dents or other damage.

4. This step inspects for a faulty release bearing.

5. This step inspects for a worn or damage diaphragm spring.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Low clutch pedal or pedal stays on the floor.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 | Inspect to see if the master cylinder pushrod has fallen off the clutch pedal. Has the master cylinder pushrod fallen off the clutch pedal? | Go to Step 3 | Go to Step 4
3 | Correctly install the master cylinder pushrod. Refer to Clutch Master Cylinder Replacement . Did you find and repair the condition? | System OK | Go to Step 4
4 | Inspect the reservoir for fluid. Is there fluid in the reservoir? | Go to Step 6 | Go to Step 5
5 | Inspect the clutch hydraulic line for bursting or leaking line. Did you find and correct the condition? | Go to Step 12 | Go to Step 6
6 | Inspect the master cylinder for being faulty. Is the master cylinder faulty? | Go to Step 7 | Go to Step 8
7 | Replace the master cylinder. Refer to Clutch Master Cylinder Replacement . Did you find and repair the condition? | Go to Step 12 | Go to Step 8
8 |

1. Remove the transmission. Refer to Transmission Replacement .
2. Inspect the clutch actuator for binding.

Did you find and repair the condition?

Go to Step 12

Go to Step 9

9 | Inspect the clutch release bearing. Refer to Clutch Actuator Cylinder Replacement . Did you find and repair the condition? | Go to Step 12 | Go to Step 10
10 | Inspect the clutch diaphragm spring. Did you find and repair the condition? | Go to Step 12 | Go to Step 11
11 | Replace the clutch pressure plate. Refer to Clutch Pressure and Driven Plate Replacement . Did you find a repair the condition? | Go to Step 12 | Go to Step 1
12 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 1