For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Balance Shaft Cover Nut and Bolt | 13 N·m | 115 lb in
Balance Shaft Driven Sprocket Bolt (left hand thread)

- First Pass

40 N·m

30 lb ft

- Final Pass

45 degrees

Balance Shaft to Housing Bolts 8 mm hex

- First Pass

10 N·m

89 lb in

- Final Pass

40 degrees

Balance Shaft Housing Bolts 10 mm hex

- First Pass

15 N·m

11 lb ft

- Final Pass

40 degrees

Balance Shaft to Block Bolts 13 mm hex

- First Pass

25 N·m

18 lb ft

- Final Pass

70 degrees

Balance Shaft to Block Bolts 15 mm hex | 53 N·m | 39 lb ft
Balance Shaft to Block Bolts 18 mm hex

- First Pass

40 N·m

30 lb ft

- Final Pass

60 degrees

Camshaft (exhaust) Rear Cover | 14 N·m | 124 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sprocket to the Camshaft Bolt | 70 N·m | 52 lb ft
Connecting Rod Nuts

- First Pass

25 N·m

18 lb ft

- Final Pass

80 degrees

Coolant Bleeder Valve | Fully Driven, Seated , Not Stripped
Coolant Outlet to Cylinder Head | 26 N·m | 19 lb ft
Coolant Pump Cover to the Block | 26 N·m | 19 lb ft
Coolant Pump to the Coolant Pump Cover | 14 N·m | 124 lb in
Coolant Pump to the Timing Chain Housing | 26 N·m | 19 lb ft
Crankshaft Balancer to the Crankshaft

- First Pass

175 N·m

129 lb ft

- Final Pass

90 degrees

Crankshaft Bearing Cap Bolts

- First Pass

20 N·m

15 lb ft

- Final Pass

90 degrees

Crankshaft Position Sensor to Block | 9 N·m | 80 lb in
Cylinder Head Bolts | Refer to Procedure
Engine Coolant Air Bleed Pipe | 14 N·m | 124 lb in
Engine Coolant Air Bleed Pipe Nut | 42 N·m | 31 lb ft
Engine Coolant Temperature Sensor to the Coolant Outlet | 11 N·m | 97 lb in
Engine Lift Bracket | 96 N·m | 68 lb ft
EVAP Canister Purge Valve Solenoid Bracket Bolt | 8 N·m | 72 lb in
Exhaust Manifold to the Cylinder Head Nuts | 42 N·m | 31 lb ft
Exhaust Manifold to the Cylinder Head Studs | 11 N·m | 97 lb in
Exhaust Manifold Upper Heat Shield to the Manifold Bolts | 26 N·m | 19 lb ft
Flywheel to the Crankshaft

- First Pass

30 N·m

22 lb ft

- Final Pass

45 degrees

Front Cover to the Timing Chain Housing | 12 N·m | 106 lb in
Fuel Pipe Bracket to the Camshaft Housing

- First Pass

15 N·m

11 lb ft

- Final Pass

30 degrees

Fuel Pipe to the Fuel Rail Nut | 30 N·m | 22 lb ft
Fuel Rail to the Camshaft Housing | 26 N·m | 19 lb ft
Ignition Coil and Module Assembly to the Camshaft Housings | 22 N·m | 16 lb ft
Intake Manifold to the Cylinder Head Bolts/Nuts | 24 N·m | 18 lb ft
Intake Manifold to the Cylinder Head Studs | 11 N·m | 97 lb in
Knock Sensor | 20 N·m | 15 lb ft
Oil/Air Separator To Block Bolts | 24 N·m | 18 lb ft
Oil Dipstick Tube Bolt/Screw | 8 N·m | 71 lb in
Oil Filter Connector to the Block | 29 N·m | 21 lb ft
Oil Filter to the Block | 3/4 to one complete turn after gasket contact
Oil Pan Bolts | 24 N·m | 18 lb ft
Oil Pan Bolts, Second Set | 12 N·m | 106 lb in
Oil Pan Drain Plug | 26 N·m | 19 lb ft
Oil Pan Studs | 26 N·m | 19 lb ft
Oil Passage Plug Bolt | 30 N·m | 22 lb ft
Oil Passage Plugs, Block 1/8x27 | 10 N·m | 89 lb in
Oil Passage Plugs, 3/8x18 | 30 N·m | 22 lb ft
Oil Passage Plugs, 1/4x18 | 20 N·m | 15 lb ft
Oil Pressure Switch | 14 N·m | 124 lb in
Oil Pump to the Balance Shaft Housing (Long Bolts) | 12 N·m | 106 lb in
Oil Pump to the Balance Shaft Housing (Short Bolts) | 10 N·m | 89 lb in
Oxygen Sensor To Exhaust Manifold | 42 N·m | 31 lb ft
Powersteering Pipe to the Pump Nut | 27 N·m | 20 lb ft
Powersteering Pump to the Cam Carrier Bolts | 26 N·m | 19 lb ft
Rear Crankshaft Seal Housing to Block | 12 N·m | 106 lb in
Spark Plugs to the Cylinder Head | 18 N·m | 13 lb ft
Starter to the Block Bolt | 90 N·m | 66 lb ft
Tensioner to Tensioner Bracket Nut | 54 N·m | 40 lb ft
Throttle Body to the Intake Manifold | 10 N·m | 89 lb in
Thrust Plate to the Balance Shaft Housing | 13 N·m | 115 lb in
Timing Chain Housing to the Block Bolts/Studs | 29 N·m | 21 lb ft
Timing Chain Housing to the Camshaft Housings | 26 N·m | 19 lb ft
Timing Chain Tensioner to Housing | 10 N·m | 89 lb in

Application | Specification
--- | ---
Metric | English
Camshaft Housing Bolt (First Pass) | 15 N·m | 11 lb ft

- Final Pass

90 degrees

Camshaft Housing Cover Bolt (First Pass) | 15 N·m | 11 lb ft

- Final Pass

30 degrees

Camshaft Sprocket Bolt | 70 N·m | 52 lb ft
Crankshaft Balancer Bolt (First Pass) | 175 N·m | 129 lb ft

- Final Pass

90 degrees

Drive Belt Tensioner Bolt | 54 N·m | 40 lb ft
Engine Front Cover Bolt | 12 N·m | 106 lb in
Engine Mounting Bracket Adapter Bolt (First Pass) | 110 N·m | 81 lb ft

- Final Pass

90 degrees

Engine Mount Bracket to Engine (Side) Bolt | 58 N·m | 43 lb ft
Engine Mount Bracket to Engine (Front) Bolt | 102 N·m | 75 lb ft
Engine Mount Bracket to Transaxle Bolt | 75 N·m | 55 lb ft
Engine Mount Nut | 66 N·m | 49 lb ft
Engine Mount Strut Bolt (First Pass) | 100 N·m | 74 lb ft
Engine Mount to Bracket Bolt | 130 N·m | 96 lb ft

- Final Pass

90 degrees

Engine Mount Strut Bracket Bolt | 66 N·m | 49 lb ft
Engine to Transmission Brace Bolt | 50 N·m | 37 lb ft
Flywheel Bolt (First Pass) | 30 N·m | 22 lb ft

- Final Pass

45 degrees

Fuel Rail to Camshaft Housing Bolt | 26 N·m | 19 lb ft
Ignition Coil and Module Cover Bolt (First Pass) | 15 N·m | 11 lb ft

- Final Pass

30 degrees

Intake Manifold Bolt/Nut | 24 N·m | 18 lb ft
Oil/Air Separator Bolt | 24 N·m | 18 lb ft
Oil Filter Adapter | 29 N·m | 21 lb ft
Oil Level Indicator Tube Bolt | 8 N·m | 72 lb in
Oil Pan Drain Bolt | 26 N·m | 19 lb ft
Oil Pan to Seal Housing Bolt | 12 N·m | 106 lb in
Oil Pan to Timing Chain Housing Bolt | 26 N·m | 19 lb ft
Oil Pump Cover Bolt | 54 N·m | 40 lb ft
Power Steering Pump Bolt | 26 N·m | 19 lb ft
Timing Chain Housing Bolt

- M8 x 1.25 x 25

26 N·m

19 lb ft

- M8 x 1.55 x 55

50 N·m

37 lb ft

- M10 x 1.25 x 35

29 N·m

21 lb ft

- M8 x 1.25 x 80

24 N·m

18 lb

- M8 x 1.24 x 22

24 N·m

18 lb ft

- M6 x 1.00 x25

12 N·m

106 lb in

Timing Chain Housing Nut | 26 N·m | 19 lb ft
Timing Chain Tensioner Bolt | 10 N·m | 89 lb in
Transmission Mount Lower Nut | 44 N·m | 60 lb ft
Transmission Mount Thru Bolt | 55 N·m | 75 lb ft