For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the hood side bumper (1) from the fender by sliding the bumper rearward.
3. Remove the adjustable front hood bumper (1) from the radiator support by rotating counterclockwise.

### Installation Procedure

1. Install the adjustable front hood bumper (1) to the radiator support by rotating clockwise.
2. Install the hood side bumper (1) to the fender.
3. Adjust the hood height by rotating the front hood bumpers clockwise/counterclockwise until the hood is flush with the front fender.