For 1990-2009 cars

### Removal Procedure

1. Remove the coat hook screw cover.

Pry the cover off with a flat-bladed tool.

2. Remove the coat hook screw (3).
3. Remove the coat hook (4).

### Installation Procedure

1. Align the coat hook with the backing plate.
2. Install the coat hook (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the coat hook screw (3).

Tighten
Tighten the coat hook screw to 1.0 N·m (9 lb in).

4. Install the coat hook screw cover.

Press the cover into place.