For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the center console. Refer to Front Floor Console Replacement in Instrument Panel, Gages, and Console.
3. Disconnect the electrical connector from the shift lock control for the automatic transmission (AT).
4. Remove both ends of the AT shift lock control from pivot points (1).

### Installation Procedure

1. Install the upper clip of the AT shift lock control onto the upper pivot point, and the lower clip onto the lower pivot point.
2. Install the center console. Refer to Front Floor Console Replacement in Instrument Panel, Gages, and Console.
3. Connect the electrical connector to the AT shift lock control.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.