For 1990-2009 cars

### Removal Procedure

1. Remove the wheelhouse splash shield. Refer to Wheelhouse Splash Shield Replacement .
2. Remove the front fender insulator retainers.

Pry outward with a flat-bladed tool.

3. Remove the front fender insulator.

### Installation Procedure

1. Install the front fender insulator.
2. Install the front fender insulator retainers.

Ensure the retainers lock into place.

3. Install the front wheelhouse panel liner. Refer to Wheelhouse Splash Shield Replacement .