For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rocker panel molding screws.
3. Use the J 38778 to release the rocker panel retainers.
4. Remove the rocker panel molding from the rocker.

### Installation Procedure

1. Position the rocker panel molding to the rocker.
2. Press the rocker panel molding to the rocker until the retainers are fully seated.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rocker panel molding screws.

Tighten
Tighten the rocker panel molding screws to 2 N·m (18 lb in).

4. Lower the vehicle.