For 1990-2009 cars

# Warranty Admin. - November, 2000 Labor Time Guide Updates

Subject: | November, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

#### LTG Update - A/B Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
BRACKET, TORQUE TUBE, MOUNTING - REPLACE | N | F1295 | -- | -- | -- | -- | -- | 0.4
OIL SEAL, AXLE SHAFT - REPLACE |  |  |  |  |  |  |  |

- FRONT AXLE

- RIGHT

N

F1600

--

--

--

--

--

1.1

- LEFT

N

F1601

--

--

--

--

--

1.1

- BOTH

N

F1607

--

--

--

--

--

1.9

SEAL, AXLE SHAFT OIL - REPLACE

- PART GP: 5.822

- REAR AXLE

- RIGHT

R

F1610

--

--

--

--

--

1.0

- LEFT

R

F1611

--

--

--

--

--

1.0

- BOTH

R

F1617

--

--

--

--

--

1.7

SEAL, PINION SHAFT OIL - REPLACE

- PART GP: 5.469

- INC: Pinion housing o-ring seal replacement

- REAR DIFFERENTIAL

R

F2023

--

--

--

--

--

1.2

VALVE ASSEMBLY, LIMITED SLIP DIFFERENTIAL CLUTCH PUMP CHECK - REPLACE

- NOTE: This labor is for check valve and or "O" ring seal

N

F2790

--

--

--

--

--

0.4

SENSOR, TRANSFER CASE SPEED - REPLACE

- NOTE: No Change to "POLICY" or "NOTE"

R

K4155

--

--

--

--

--

0.4

- No Change to "ADD" Condition

SEAL, TRANSFER CASE OIL - REPLACE |  |  |  |  |  |  |  |

- FRONT

R

K4162

--

--

--

--

--

1.4

- REAR

K4163

--

--

--

--

--

0.4

PLUG, TRANSFER CASE DRAIN - REPLACE | R | K4290 | -- | -- | -- | -- | -- | 0.3
PLUG, TRANSFER CASE FILL - REPLACE | N | K4291 | -- | -- | -- | -- | -- | 0.3
PLUG AND/OR SEAL, TRANSMISSION FLUID DRAIN - REPLACE

- NOTE: Applies to Auto Trans 4T65E

N

K6150

--

--

--

--

--

0.2

*IND: N - New/R - Revised

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CONTROL ASSEMBLY, RADIO - R&R OR REPLACE

- PART GP: 9.650

- POLICY: S

N

R0765

--

--

--

0.3

0.3

- NOTE: This operation is to be used with AC-Delco Form 1078 when radio is sent out for repair.

- NOTE: Also known as rear audio control.

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - C/K New Body Style

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 |  |  |  |  |  |

- PICKUP

--

--

--

1.2

1.2

1.2

- YUKON/TAHOE

--

--

--

--

1.4

1.4

- SUBURBAN/YUKON/XL

--

--

--

--

1.4

1.4

- DENALI

--

--

--

--

--

2.0

- CAB/CHASSIS

--

--

--

--

--

1.2

ADD: |  |  |  |  |  |  |  |

- A- To Install Senior West Coast Type Exterior Mirrors 9F8 (Pickup and Chassis Cab Only)

--

--

--

0.4

0.4

0.4

- DG5 (Chassis Cab Only)

--

--

--

0.4

0.4

0.4

- B- To Install Running Boards

- Without Rear A/C and/Or Heat (Tahoe, Suburban, Yukon, Yukon XL)

--

--

--

--

1.1

1.1

- With Rear A/C and/Or Heat (Tahoe, Suburban, Yukon, Yukon XL)

--

--

--

--

1.5

1.5

Pickups with RPO Y91 | R |  | -- | -- | -- | -- | 1.1 | 1.1

- C- To Install Tonneau Cover

- Pickups With E95

--

--

--

--

0.3

0.3

- D- To Install On-Star Antenna and Check System Operation

--

--

--

--

0.2

0.2

- E- To Check/Aim Headlights (For Incomplete Vehicles Where 3rd Position of Vin is B or D)

--

--

--

--

--

0.1

- F- To Torque All Front and Rear Lug Nuts (With Dual Rear Wheels RPO R05 Only)

--

--

--

--

--

0.1

- G- To Install Wheel Covers With RPO N67, N83, N90, P06, PF4, or R05

--

--

--

--

--

0.1

*IND: N - New/R - Revised

#### LTG Update - E/J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CABLE AND/OR "O" RING, THROTTLE VALVE CONTROL (TV) - REPLACE

- INC: Clean oil pan and service screen

- NOTE: Applies to Auto Trans 03-72LE

K6200

- 2WD

1.3

1.3

1.3

1.3

1.3

1.3

- 4WD

R

1.4

1.4

1.4

1.7

1.7

1.7

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
VALVE, EVAPORATIVE EMISSION CANISTER VENT SOLENOID - REPLACE | N | J6441 | -- | -- | 2.7 | 2.9 | 2.9 | 2.9

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MODULE, SDM (SUPPLEMENTAL INFLATABLE RESTRAINT SYSTEM CONTROL MODULE) - REPLACE | R | C8817 | 0.7 | 0.7 | 0.9 | 0.9 | 1.2 | 1.2

- No Change to "ADD" Condition

INSTRUMENT PANEL CLUSTER COMPONENETS (DIGITAL/ELECTRO MECHANICAL) - R&R OR REPLACE

- POLICY: S

INSTRUMENT PANEL CLUSTER ASSEMBLY |  | N4180 |  |  |  |  |  |

- PONTIAC

0.6

0.8

0.8

0.8

0.2

0.2

- OLDSMOBILE

0.6

0.6

0.4

0.4

- BUICK

R

0.9

0.5

0.5

0.5

0.8

0.8

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SEAT AND/OR INSULATOR, REAR SPRING (UPPER AND/OR LOWER) - REPLACE

- PART GP: 7.545

N

RIGHT |  | E5050 | 0.6 | 0.6 | 0.6 |  |  |
LEFT |  | E5051 | 0.6 | 0.6 | 0.6 |  |  |
BOTH |  | E5057 | 0.9 | 0.9 | 0.9 |  |  |
*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CELLULAR MOBILE TELEPHONE/NAVIGATION SYSTEM COMPONENTS - REPLACE

- NOTE: No Change to "POLICY", or Labor Operations R5111, R5114 thru R5130, or R5132 thru R5153

HANDSET | R | R5113 | 0.1 | 0.1 | 0.1 | 0.1 | 0.2 | 0.2
MODULE, CELLULAR (RPO UV8) | N | R5131 | -- | -- | -- | -- | 0.3 | 0.3

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CELLULAR MOBILE TELEPHONE/NAVIGATION SYSTEM COMPONENTS - REPLACE

- NOTE: No Change to "POLICY", or Labor Operations R5111, R5114 thru R5130, or R5132 thru R5145

HANDSET | R | R5113 | 0.1 | 0.1 | 0.1 | 0.1 | 0.2 | 0.2
MODULE, CELLULAR (RPO UV8) | N | R5131 | -- | -- | -- | -- | 0.3 | 0.3

- No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
DOOR (VALVE), MODULE - REPLACE

- NOTE: No Change to "INC", "PART GP", or Labor Operations D1860, D1870 or D1877

UPPER AND/OR LOWER MODE |  | D1867 |  |  |  |  |  |
MALIBU & CUTLASS | R |  | -- | 3.4 | 3.4 | 3.4 | 3.4 | 3.4
ACHIEVA & SKYLARK |  |  | 1.5 | 1.5 | 1.5 |  |  |
GRAND AM & ALERO |  |  | 1.5 | 1.5 | 1.5 | 2.6 | 2.6 | 2.6

- No Change to "ADD" Condition

CORE, EVAPORATOR - REPLACE |  | D3320 |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
GRAND AM | R |  | 2.1 | 2.1 | 2.1 | 4.9 | 4.9 | 4.9
ACHIEVA - 4 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
ACHIEVA - 6 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
ALERO | R |  | -- | -- | -- | 4.8 | 4.8 | 4.8
SKYLARK - 4 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |
SKYLARK - 6 CYL |  |  | 2.1 | 2.1 | 2.1 |  |  |

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
FRAME, ENGINE - REPLACE

- NOTE: No Change to "NOTEs" or "PART GP"

COMPLETE |  | E1707 |  |  |  |  |  |
EXC IMPALA |  |  | 2.3 | 2.3 | 2.8 | 2.8 | 2.8 | 2.8
IMPALA | R |  | -- | -- | -- | -- | 2.3 | 2.3
GENERATOR ASSEMBLY - REPLACE

- NOTE: No Change to "NOTE" or "PART GP"

J4100

ENGINE CODE M, T, J AND E |  |  |  |  |  |  |  |
EXC CHEVROLET |  |  | 1.0 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
CHEVROLET - LUMINA |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
CHEVROLET - IMPALA AND MONTE CARLO |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.5 | 0.5
ENGINE CODE X |  |  | 2.0 | 2.0 |  |  |  |
ENGINE CODE K, L AND 1 |  |  |  |  |  |  |  |
CHEVROLET |  |  | -- | -- | 0.5 | 0.5 | 0.5 | 0.5
PONTIAC, OLDSMOBILE AND BUICK | N |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
ENGINE CODE H |  |  | -- | -- | -- | 1.8 | 1.8 | 1.8

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
COVER AND/OR GASKET, DIFFERENTIAL - REPLACE

- PART GP: 5.398

REAR DIFFERENTIAL |  |  |  |  |  |  |  |
RIGHT | N | F2004 | -- | 1.8 | 1.8 | 1.8 | 1.8 | 1.8
LEFT | N | F2005 | -- | 1.9 | 1.9 | 1.9 | 1.9 | 1.9
REAR | N | F2006 | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
*IND: N - New/R - Revised