For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the hoses from the EVAP canister.
3. Remove the attaching bolt from the EVAP canister retainer .
4. Remove the EVAP canister and the retainer.

Notice: The EVAP canister may have released carbon particles which caused this part to fail and may cause damage to other components. Check the EVAP canister for loose carbon before returning the vehicle to service.

5. Remove the EVAP canister retainer from the canister.

### Installation Procedure

1. Snap the EVAP canister retainer onto the EVAP canister.
2. Install the end of the EVAP canister into the tab on the body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the attaching bolt to the EVAP canister retainer .

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Reconnect the hoses to the EVAP canister.
5. Lower the vehicle.