For 1990-2009 cars

## Coolant Heater Cord Replacement 2.2L (L61)

### Removal Procedure

1. Disconnect the engine coolant heater cord (1).
2. Remove the clips from the engine mount and surge tank.

### Installation Procedure

1. Install the clips from the engine mount and surge tank.
2. Connect the engine coolant heater cord (1).

## Coolant Heater Cord Replacement 3.4L (LA1)

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the engine engine coolant heater cord from the engine engine coolant heater.
3. Remove the engine engine coolant heater cord straps.
4. Disconnect the upper engine engine coolant heater cord from the diagonal brace strap.
5. Remove the engine engine coolant heater cord.

### Installation Procedure

1. Install the engine engine coolant heater cord.
2. Connect the engine engine coolant heater cord to the engine engine coolant heater.
3. Lower the vehicle.
4. Route the engine coolant heater cord to the air cleaner housing.
5. Install the new engine engine coolant heater cord straps.