For 1990-2009 cars

### Removal Procedure

1. Open the sunshade.
2. Close the sunroof glass panel.
3. Remove the sunroof glass panel screws.
4. Remove the sunroof glass panel.

### Installation Procedure

1. Install the sunroof glass panel into the roof opening.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the sunroof glass panel screws (2).

Tighten
Tighten the sunroof glass panel screws to 4 N·m (35 lb in).

3. Adjust the sunroof glass panel. Refer to Sunroof Window Height and Opening Fit Adjustment .