For 1990-2009 cars

### Removal Procedure

1. Remove the screws that secure the fuel tank filler pipe housing to the fuel tank filler neck.
2. Remove the fuel tank filler pipe housing by disengaging the 3 retaining lugs from the quarter panel.

### Installation Procedure

1. Install the fuel tank filler pipe housing. Fully engage the 3 retaining lugs.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws in order to secure the fuel tank filler pipe housing to the fuel tank filler neck.

Tighten
Tighten the tank fuel filler pipe housing screws to 2 N·m (18 lb in).