For 1990-2009 cars

Caution: The tilt spring and the spring guide are under pressure. The tilt spring and the spring guide may become a projectile. Secure the spring with locking pliers during removal. Secure the spring with locking pliers during installation. Bodily injury may result during removal and installation of the tilt spring and the spring guide. Always use caution during removal and installation of the tilt spring and the spring guide.

1. Use the tilt lever to move the tilt column into the UP position.
2. Pry the tilt spring (1) upward until a bulge occurs and most of the spring tension is removed.
3. Secure the tilt spring (1) with locking pliers.
4. Continue prying the tilt spring (1) until the tilt spring disengages from the post on the steering column support assembly, the steering column housing, and the bearing assembly.
5. Remove the tilt spring guide (1) from the tilt spring (2).