For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement .
2. Disconnect the cruise control cable (2) from the throttle body (3) and the accelerator bracket (1).
3. Disconnect the accelerator control cable (3) from the throttle body (4) and accelerator bracket (1).
4. Remove the 2 accelerator bracket nuts (3).
5. Remove the accelerator bracket (2) from the throttle body (1).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the accelerator bracket (2) on the throttle body (1).

Tighten
Tighten the accelerator bracket nuts to 10 N·m (89 lb in).

2. Connect the accelerator control cable (3) to the throttle body (4) and accelerator bracket (1).
3. Connect the cruise control cable(2) from the throttle body(3) and the accelerator bracket (1).
4. Install the air cleaner outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement .