For 1990-2009 cars

## Rear Compartment Release Switch Replacement Pontiac

### Removal Procedure

1. Remove the rear compartment release switch from the front door panel, using a small flat-bladed tool to release the retainers.
2. Disconnect the electrical connector from the rear compartment release switch.

### Installation Procedure

1. Connect the electrical connector to the rear compartment release switch.
2. Install the rear compartment release switch to the front door panel, pressing into place until fully seated.

## Rear Compartment Release Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the rear compartment release switch from the front door panel, using a small flat-bladed tool to release the retainers.
2. Disconnect the electrical connector from the rear compartment release switch.

### Installation Procedure

1. Connect the electrical connector to the rear compartment release switch.
2. Install the rear compartment release switch to the front door panel, pressing into place until fully seated.