For 1990-2009 cars

#### Tools Required

J 44641 Crankshaft Rear Oil Seal Remover

1. Install the button of J 44641 into the crankshaft.
2. Press the jaws of J 44641 into the felt portion of the seal far enough to engage the inner lip of the seal.
3. While holding the jaws of J 44641 tightly to the seal's inner sleeve, tighten the jaw bolts.
4. Remove the crankshaft rear oil seal using the J 44641 .