For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the OFF position.
2. Remove the right insulator panels. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument panel, Gages, and Console.
3. Slide the body control module (BCM) from the bracket.
4. Disconnect the BCM connectors from the BCM.
5. Remove the BCM (2).

### Installation Procedure

1. Connect the BCM connectors to the BCM.
2. Install the BCM (2) to the bracket.
3. Program the BCM. Refer to Body Control Module (BCM) Programming/RPO Configuration .
4. Install the right insulator panels. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument panel, Gages, and Console