For 1990-2009 cars

## Fog Lamp Switch Replacement Pontiac

### Removal Procedure

1. Place the ignition switch in the OFF position.
2. Remove the instrument panel (IP) switch trim plate from the instrument panel (IP) using a small flat-bladed tool.
3. Disconnect the electrical connectors.
4. Disengage the retaining tabs. Remove the fog lamp switch.

### Installation Procedure

1. Install the fog lamp switch to the trim plate by pressing into place until fully seated.
2. Connect the electrical connectors to the switches.
3. Install the IP switch trim plate to the IP opening. Press the trim plate into place until fully seated.

## Fog Lamp Switch Replacement Oldsmobile

### Removal Procedure

1. Place the ignition switch in the OFF position.
2. Use a small flat-bladed tool to remove the outer air outlet from the instrument panel (IP).
3. Disconnect the electrical connectors (1) from the switches.
4. Remove the fog lamp switch (1) by disengaging the retainers.

### Installation Procedure

1. Install the fog lamp switch (1) to the IP outer air outlet. Press the switch into place until fully seated.
2. Connect the electrical connectors (1) to the switches.
3. Install the IP outer air outlet. Press the outlet into place until fully seated.