For 1990-2009 cars

### Removal Procedure

1. Remove the starter. Refer to Starter Motor Replacement in Engine Electrical.
2. Disconnect the crankshaft position (CKP) sensor harness connector.
3. Remove the CKP sensor bolt.
4. Remove the CKP sensor.

### Installation Procedure

1. Inspect the CKP sensor O-ring and lubricate with a mineral based grease.
2. Gently insert the CKP sensor into the block.