For 1990-2009 cars

1. Connect the passenger yellow 2-way connector (3) located above the RH I/P wiring harness junction block.
2. Install the connector position assurance (CPA (2) to the passenger yellow 2-way connector (3).
3. Install the RH I/P wiring harness junction block access panel.
4. Connect the driver yellow 2-way connector (1) located above the LH I/P wiring harness junction block.
5. Install the connector position assurance (CPA) (2) to the driver yellow 2-way connector (1).
6. Install the AIR BAG Fuse to the LH I/P wiring harness junction block.
7. Install the LH I/P wiring harness junction block access panel.
8. Staying well away from both air bags, turn ON the ignition.

8.1. | The AIR BAG warning lamp will flash seven times.

8.2. | The AIR BAG warning lamp will then turn OFF.

9. Perform A Diagnostic System Check - SIR if the AIR BAG warning lamp does not operate as described.