For 1990-2009 cars

#### Tools Required

J 36513 Gear and Bearing Separator Plate

Important:

• | Only remove the bearings if replacing the bearings. Do not use the bearings again after removal.

• | You must also replace the race for the bearing being replaced.

1. Inspect the bearing for damage or wear. Refer to Bearings and Spacers Cleaning and Inspection .
2. Using a hydraulic press and the J 36513 (1), remove the input shaft bearing.
3. Remove the input shaft oil deflector using a suitable prying tool.
4. Discard the input shaft oil deflector after removal.