For 1990-2009 cars

### Removal Procedure

1. Remove the radio antenna.
2. Pull back the rear compartment trim panel for access.
3. Disconnect the antenna cable (2) from the radio antenna bracket (3).
4. Remove the screws from the radio antenna cable.
5. Remove the radio antenna bracket (3).
6. Pull the radio antenna bezel (1) from the quarter panel.

### Installation Procedure

1. Press the radio antenna bezel (1) into the quarter panel opening.
2. Position the radio antenna bracket (3) to the inner quarter panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the radio antenna cable screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Connect the antenna cable (2) to the radio antenna bracket (3).
5. Install the rear compartment trim panel.
6. Install the radio antenna.