For 1990-2009 cars

### Removal Procedure

1. Using a small flat-bladed tool, carefully pry at the rear edge (furthest from the windshield) of the lamp lens (2) to release the retaining tabs, then remove the lens from the rearview mirror.
2. Carefully remove the bulb (1) from the socket.

### Installation Procedure

1. Install the bulb (1) to the socket.
2. Align and insert the forward edge (nearest the windshield) of the lamp lens (2) into place, then press the rear edge into place to secure the lens.