For 1990-2009 cars

Table 1: | C101
Table 2: | Automatic Transaxle C102
Table 3: | C120 (LA1 Only)
Table 4: | C130 (LA1 Only)
Table 5: | C200
Table 6: | C300
Table 7: | C306
Table 8: | C400
Table 9: | C413 (1 of 3)
Table 10: | C413 (2 of 3)
Table 11: | C413 (3 of 3)
Table 12: | C500
Table 13: | C501
Table 14: | C600
Table 15: | C700
Table 16: | C800

#### C101

Connector Part Information |

• | 12177081

• | 10-Way F Global Terminal 150 Series (BLK)

Connector Part Information

• | 12045808

• | 10-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | -- | -- | Not Used | A | -- | -- | Not Used
B | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile) | B | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
C | GRY/BLK | 87 | Cruise Control Switch Signal (RESUME/ACCEL) | C | GRY/BLK | 87 | Cruise Control Switch Signal (RESUME/ACCEL)
D | DK BLU | 84 | Cruise Control Switch Signal (SET/COAST) | D | DK BLU | 84 | Cruise Control Switch Signal (SET/COAST)
E | RED | 228 | Windshield Washer Pump Motor Feed | E | RED | 228 | Windshield Washer Pump Motor Feed
F | BLK/WHT | 99 | Windshield Washer Fluid Level Sensor Signal | F | BLK/WHT | 99 | Windshield Washer Fluid Level Sensor Signal
G | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output | G | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output
H | GRY | 397 | Cruise Control Switch Output (ON) | H | GRY | 397 | Cruise Control Switch Output (ON)
J-K | -- | -- | Not Used | J-K | -- | -- | Not Used

#### Automatic Transaxle C102

Connector Part Information |

• | 12160493

• | 20-Way F Micro-Pack 100 Series (GRY)

Connector Part Information

• | 12160782

• | 20-Way M Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | LT GRN | 1222 | Shift Solenoid A Output | A | LT GRN | 1222 | Shift Solenoid A Output
B | YEL/BLK | 1223 | Shift Solenoid B Output | B | YEL | 1223 | Shift Solenoid B Output
C | RED/BLK | 1228 | Transaxle Force Motor Feed | C | PPL | 1228 | Transaxle Force Motor Feed
D | LT BLU/WHT | 1229 | Transaxle Force Motor Return | D | LT BLU | 1229 | Transaxle Force Motor Return
E | PNK | 1039 | Fuse Output, Ignition 1 | E | RED | 839 | Fuse Output, Ignition 1
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | YEL/BLK | 1227 | Transaxle Temperature Sensor Signal | L | BRN | 1227 | Transaxle Temperature Sensor Signal
M | BLK/WHT | 2762 | Sensor Ground | M | GRY | 452 | Sensor Return
N | PNK | 1224 | Transaxle Pressure Switch Signal (Bit 1) | N | PNK | 1224 | Transaxle Pressure Switch Signal (Bit 1)
P | RED | 1226 | Transaxle Pressure Switch Signal (Bit 3) | P | ORN | 1226 | Transaxle Pressure Switch Signal (Bit 3)
R | DK BLU | 1225 | Transaxle Pressure Switch Signal (Bit 2) | R | DK BLU | 1225 | Transaxle Pressure Switch Signal (Bit 2)
S | RED/BLK | 1230 | Transaxle Input Speed Sensor Signal | S | BLK | 1230 | Transaxle Input Speed Sensor Signal
T | BRN | 418 | TCC Solenoid Output (Pulse Width) | T | TAN | 418 | TCC Solenoid Output (Pulse Width)
U | YEL | 657 | TCC Oil Pressure Switch Signal | U | WHT | 1804 | TCC Oil Pressure Switch Signal
V | DK BLU/WHT | 1231 | Transaxle Input Speed Sensor Return | V | DK GRN | 1231 | Transaxle Input Speed Sensor Return
W | -- | -- | Not Used | W | -- | -- | Not Used

#### C120 (LA1 Only)

Connector Part Information |

• | 12052644

• | 2-Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12162343

• | 2-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 452 | Sensor Return | A | BLK/WHT | 2761 | --
B | YEL | 410 | Coolant Temperature Sensor Signal | B | YEL | 410 | Coolant Temperature Sensor Signal

#### C130 (LA1 Only)

Connector Part Information |

• | 12065425

• | 10-Way F Global Terminal 150 Series (BLK)

Connector Part Information

• | 12048253

• | 10-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 1744 | Fuel Injector 1 Output | A | BLK | 1744 | Fuel Injector 1 Output
B | LT GRN/BLK | 1745 | Fuel Injector 2 Output | B | LT GRN/BLK | 1745 | Fuel Injector 2 Output
C | PNK/BLK | 1746 | Fuel Injector 3 Output | C | PNK/BLK | 1746 | Fuel Injector 3 Output
D | PNK | 839 | Fuse Output, Ignition 1 | D | PNK | 639 | Fuse Output, Ignition 1
E | ORN/BLK | 469 | MAP Sensor Return | E | ORN/BLK | 469 | MAP Sensor Return
F | BRN | 2704 | -- | F | GRY | 416 | --
G | LT GRN | 432 | Manifold Absolute Pressure Sensor Signal | G | LT GRN | 432 | Manifold Absolute Pressure Sensor Signal
H | YEL/BLK | 846 | Fuel Injector 6 Output | H | YEL/BLK | 846 | Fuel Injector 6 Output
J | BLK/WHT | 845 | Fuel Injector 5 Output | J | BLK/WHT | 845 | Fuel Injector 5 Output
K | LT BLU/BLK | 844 | Fuel Injector 4 Output | K | LT BLU/BLK | 844 | Fuel Injector 4 Output

#### C200

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15317538

• | 18-Way M Global Terminal Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary) | A1 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
A2-A3 | -- | -- | Not Used | A2-A3 | -- | -- | Not Used
A4 | BLK | 250 | Ground | A4 | BLK | 250 | Ground
A5 | BLK | 250 | Ground | A5 | BLK | 250 | Ground
A6 | -- | -- | Not Used | A6 | -- | -- | Not Used
A7 | ORN/BLK | 556 | Steering Wheel Position Sensor Return | A7 | ORN/BLK | 556 | Steering Wheel Position Sensor Return
A8 | GRY | 1056 | Steering Wheel Position Sensor Feed-5 Volt Reference | A9 | GRY | 1056 | Steering Wheel Position Sensor Feed-5 Volt Reference
A9 | LT BLU | 1059 | Steering Wheel Position Sensor Signal | A9 | LT BLU | 1059 | Steering Wheel Position Sensor Signal
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BLK/WHT | 451 | Engine Control Module Ground | B2 | BLK/WHT | 451 | Engine Control Module Ground
B3 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile) | B3 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | LT GRN | 24 | Backup Lamp Feed | B5 | LT GRN | 24 | Backup Lamp Feed
B6 | -- | -- | Not Used | B6 | -- | -- | Not Used
B7 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary) | B7 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
B8 | BRN/WHT | 419 | Check Engine Indicator Lamp Output | B8 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
B9 | PPL | 1500 | Fuse Output, Ignition 0 | B9 | PPL | 1500 | Fuse Output, Ignition 0

#### C300

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12078169

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | 882 | Wheel Speed Sensor Signal, Right Rear | A | BRN | 882 | Wheel Speed Sensor Signal, Right Rear
B | WHT | 883 | Wheel Speed Sensor Return, Right Rear | B | WHT | 883 | Wheel Speed Sensor Return, Right Rear
C | BLK | 884 | Wheel Speed Sensor Signal, Left Rear | C | BLK | 884 | Wheel Speed Sensor Signal, Left Rear
D | RED | 885 | Wheel Speed Sensor Return, Left Rear | D | RED | 885 | Wheel Speed Sensor Return, Left Rear
E | BLK | 2759 | -- | E | BLK | 2759 | --
F | GRY | 2709 | -- | F | GRY | 2709 | --
G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H | LT GRN | 275 | Park/Neutral Position Switch Output | H | LT GRN | 275 | Park/Neutral Position Switch Output
J | PPL | 1589 | -- | J | PPL | 1589 | --
K | WHT | 1310 | Canister Vent Valve Solenoid Output | K | WHT | 1310 | Canister Vent Valve Solenoid Output

#### C306

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | ORN | 540 | Fuse Output, Battery | A | ORN | 540 | Fuse Output, Battery
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### C400

Connector Part Information |

• | 12015416

• | 8-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12186074

• | 8-Way M Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | ORN | 1732 | Inadvertent Power Control (12 V) | A | ORN | 1732 | Inadvertent Power Control (12 V)
B-C | -- | -- | Not Used | B-C | -- | -- | Not Used
D | BRN | 541 | Fuse Output, Ignition 3 | D | BRN | 541 | Fuse Output, Ignition 3
E | WHT | 156 | Courtesy Lamp Output | E | WHT | 156 | Courtesy Lamp Output
F | -- | -- | Not Used | F | -- | -- | Not Used
G | BLK | 750 | Ground | G | BLK | 750 | Ground
H | -- | -- | Not Used | H | -- | -- | Not Used

#### C413 (1 of 3)

Connector Part Information |

• | 12146439

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12160830

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | WHT | 883 | Wheel Speed Sensor Return, Right Rear | A1 | WHT | 883 | Wheel Speed Sensor Return, Right Rear
B | BRN | 882 | Wheel Speed Sensor Signal, Right Rear | B1 | BRN | 882 | Wheel Speed Sensor Signal, Right Rear
C | RED | 885 | Wheel Speed Sensor Return, Left Rear | C1 | RED | 885 | Wheel Speed Sensor Return, Left Rear
D | BLK | 884 | Wheel Speed Sensor Signal, Left Rear | D1 | BLK | 884 | Wheel Speed Sensor Signal, Left Rear

#### C413 (2 of 3)

Connector Part Information |

• | 12162144

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12160830

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | 241 | Fuse Output, Ignition 3 | A2 | BRN | 241 | Fuse Output, Ignition 3
B | WHT | 1310 | Canister Vent Valve Solenoid Output | B2 | WHT | 1310 | Canister Vent Valve Solenoid Output
C-D | -- | -- | Not Used | C2-D2 | -- | -- | Not Used

#### C413 (3 of 3)

Connector Part Information |

• | 15317611

• | 7-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12160830

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 150 | Ground | A3 | BLK | 550 | Ground
B | BLK/WHT | 651 | Fuel Gauge Sensor Ground | B3 | BLK | 2759 | --
C | GRY | 120 | Fuel Pump Motor Feed | C3 | GRY | 120 | Fuel Pump Motor Feed
D | PPL | 30 | Fuel Gauge Sensor Signal | D3 | PPL | 1589 | --
E | -- | -- | Not Used | E3 | -- | -- | Not Used
F | GRY/BLK | 416 | Reference Voltage Feed (5 V) | F3 | GRY | 2709 | --
G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | G3 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H | ORN/BLK | 469 | MAP Sensor Return | H3 | BLK | 2759 | --

#### C500

Connector Part Information |

• | 15304690

• | 18-Way F Global Terminal Mixed Series (GRY)

Connector Part Information

• | 15317537

• | 18-Way M Global Terminal Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor-Down Direction (Oldsmobile) | A1 | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor-Down Direction (Oldsmobile)
A1 | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor-Up Direction (Pontiac) | A1 | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor-Up Direction (Pontiac)
A2 | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor-Right Direction | A2 | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor-Right Direction
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | LT BLU | 166 | Power Window Master Switch Output-Right Front Window (UP) | A4 | LT BLU | 166 | Power Window Master Switch Output-Right Front Window (UP)
A5 | TAN | 167 | Power Window Master Switch Output-Right Front Window (DOWN) | A5 | TAN | 167 | Power Window Master Switch Output-Right Front Window (DOWN)
A6 | BLK | 550 | Ground | A6 | BLK | 550 | Ground
A7-A9 | -- | -- | Not Used | A7-A9 | -- | -- | Not Used
B1 | GRY | 8 | IP Lamp Feed (Oldsmobile) | B1 | GRY | 8 | IP Lamp Feed (Oldsmobile)
B2 | GLK | 550 | Ground | B2 | BLK | 550 | Ground
B3 | -- | -- | Not Used | B3 | -- | -- | Not Used
B4 | BRN | 141 | Fuse Output, Ignition 3 | B4 | BRN | 141 | Fuse Output, Ignition 3
B5-B7 | -- | -- | Not Used | B5-B7 | -- | -- | Not Used
B8 | ORN | 1840 | Fuse Output, Battery | B8 | ORN | 1840 | Fuse Output, Battery
B9 | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT) | B9 | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)

#### C501

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15317538

• | 18-Way M Global Terminal Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front | A1 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front
A2 | BLK | 1576 | Trunk Release Switch Output | A2 | BLK | 1576 | Trunk Release Switch Output
A3 | BLK | 550 | Ground | A3 | BLK | 550 | Ground
A4 | LT GRN | 170 | Power Window Master Switch Output, Right Rear Window (UP) | A4 | LT GRN | 170 | Power Window Master Switch Output, Right Rear Window (UP)
A5 | PPL | 171 | Power Window Master Switch Output, Right Rear Window (DOWN) | A5 | PPL | 171 | Power Window Master Switch Output, Right Rear Window (DOWN)
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | TAN | 694 | Power Door Lock Motor Feed (UNLOCK) | A8 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
A9 | GRY | 295 | Power Door Lock Motor Feed (LOCK) | A9 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
B1 | GRY | 118 | Speaker Return, Left Front | B1 | GRY | 118 | Speaker Return, Left Front
B2 | BLK | 550 | Ground | B2 | BLK | 550 | Ground
B3 | -- | -- | Not Used | B3 | -- | -- | Not Used
B4 | DK BLU | 1307 | Power Window Master Switch Output, Lockout | B4 | DK BLU | 1307 | Power Window Master Switch Output, Lockout
B5 | TAN | 167 | Power Window Master Switch Output, Right Front | B5 | TAN | 167 | Power Window Master Switch Output, Right Front
B6 | LT BLU | 166 | Power Window Master Switch Output, Right Front | B6 | LT BLU | 166 | Power Window Master Switch Output, Right Front
B7 | GRY | 8 | IP Lamp Feed | B7 | GRY | 8 | IP Lamp Feed
B8 | TAN | 201 | Speaker Feed, Left Front | B8 | TAN | 201 | Speaker Feed, Left Front
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used

#### C600

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15317538

• | 18-Way M Global Terminal Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor (DOWN) (Oldsmobile) | A1 | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor (DOWN) (Oldsmobile)
A1 | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor (UP) (Pontiac) | A1 | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor (UP) (Pontiac)
A2 | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT) | A2 | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT)
A3 | BLK | 550 | Ground | A3 | BLK | 550 | Ground
A4 | LT BLU | 166 | Power Window Master Switch Output, Right Front Window (UP) | A4 | LT BLU | 166 | Power Window Master Switch Output, Right Front Window (UP)
A5 | TAN | 167 | Power Window Master Switch Output, Right Front Window (DOWN) | A5 | TAN | 167 | Power Window Master Switch Output, Right Front Window (DOWN)
A6 | LT BLU | 395 | Door Handle Switch Signal, Right Front | A6 | LT BLU | 395 | Door Handle Switch Signal, Right Front
A7 | -- | -- | Not Used | A7 | -- | -- | Not Used
A8 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK) | A8 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
A9 | GRY | 295 | Power Door Lock Motor Feed (LOCK) | A9 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
B1 | DK GRN | 117 | Speaker Return, Right Front | B1 | DK GRN | 117 | Speaker Return, Right Front
B2 | BLK | 650 | Ground | B2 | BLK | 650 | Ground
B3 | -- | -- | Not Used | B3 | -- | -- | Not Used
B4 | BRN/DK BLU | 1307 | Power Window Master Switch Output, Lockout | B4 | BRN/DK BLU | 1307 | Power Window Master Switch Output, Lockout
B5-B6 | -- | -- | Not Used | B5-B6 | -- | -- | Not Used
B7 | GRY | 8 | IP Lamp Feed | B7 | GRY | 8 | IP Lamp Feed
B8 | LT GRN | 200 | Speaker Feed, Right Front | B8 | LT GRN | 200 | Speaker Feed, Right Front
B9 | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT) | B9 | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)

#### C700

Connector Part Information |

• | 12191689

• | 7-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 12191677

• | 7-Way M Global Terminal Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Power Door Lock Motor Feed (LOCK) | B | GRY | 295 | Power Door Lock Motor Feed (LOCK)
C | PPL | 171 | Power Window Master Switch Output, Right Rear (DOWN) | C | PPL | 171 | Power Window Master Switch Output, Right Rear (DOWN)
D | TAN | 294 | Power Door Lock Motor Feed (UNLOCK) | D | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | LT GRN | 170 | Door Window Master Switch Output, Right Rear (UP) | G | LT GRN | 170 | Door Window Master Switch Output, Right Rear (UP)
H | DK BLU | 1307 | Power Window Master Switch Output (Lockout) | H | DK BLU | 1307 | Power Window Master Switch Output (Lockout)

#### C800

Connector Part Information |

• | 12191689

• | 7-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 12191677

• | 7-Way M Global Terminal Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Power Door Lock Motor Feed (LOCK) | B | GRY | 295 | Power Door Lock Motor Feed (LOCK)
C | PPL | 169 | Door Window Master Switch Output, Left Rear (DOWN) | C | PPL | 169 | Door Window Master Switch Output, Left Rear (DOWN)
D | TAN | 294 | Power Door Lock Motor Feed (UNLOCK) | D | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | LT GRN | 170 | Door Window Master Switch Output, Right Rear (UP) | G | LT GRN | 170 | Door Window Master Switch Output, Right Rear (UP)
H | DK BLU | 1307 | Power Window Master Switch Output (Lockout) | H | DK BLU | 1307 | Power Window Master Switch Output (Lockout)