For 1990-2009 cars

### Removal Procedure

1. Disconnect negitive battery cable (2). Refer to Battery Negative Cable Disconnection and Connection .
2. Remove bolt retaining negitive cable to core support.
3. Remove tape holding positive cable and ground strap to negitive cable.
4. Remove negitive cable from retainers.
5. Raise vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Remove lower closeout panel.
7. Remove front transmission mount. Refer to Transmission Front Mount Replacement in Transmission/Transaxle-Automatic Transmission
8. Remove nut retaining ground cable to bellhousing stud.
9. Remove ground cable.

### Installation Procedure

1. Install ground cable.
2. Install nut to retain ground cable to bellhousing stud.
3. Install front transmission mount. Refer to Transmission Front Mount Replacement in Transmission/Transaxle-Automatic Transmission.
4. Install lower closeout panel.
5. Lower vehicle.
6. Install negitive cable to retainers.
7. Tape positive cable and ground strap to negitive cable.
8. Install bolt to retain ground cable to core support.
9. Connect negitive ground cable (2). Refer to Battery Negative Cable Disconnection and Connection in Engine-Engine Electrical.