For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Cruise Control Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Cruise Control
2 | Operate the vehicle within the conditions for cruise control operation. Does the cruise control system operate correctly? | -- | Go to Step 3 | Go to Cruise Control Inoperative/Malfunctioning or Cruise Control Inoperative/Malfunctioning Using J 42958 Cruise Control Tester
3 | Use a scan tool in order to command the cruise lamp ON/OFF. Does the cruise lamp respond correctly to each command? | -- | Go to Powertrain On Board Diagnostic (OBD) System Check for the 3.4L or Powertrain On Board Diagnostic (OBD) System Check for the 2.4L in Engine Controls | Go to Step 4
4 | Replace the Instrument Panel Cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console. Did you complete the replacement? | -- | System OK | Go to Step 5
5 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Diagnostic System Check - Cruise Control