For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.Refer to Battery Negative Cable Disconnection and Connection

In Engine Electrical

2. Remove the oil level indicator tube nut.
3. Remove the oil level indicator tube from the engine.

### Installation Procedure

1. Install the oil level indicator tube to the engine. Ensure that the tube assembly is fully seated in the engine.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil level indicator tube nut.

Tighten
Tighten the nut to 25 N·m (18 lb ft).

3. Connect the negative battery cable.