For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the oil pan drain plug.
3. Clean any metallic shavings from the magnetic drain plug. The plug is designed to isolate the metal particles from the engine oil and some accumulation is normal.
4. Remove the oil filter.

### Installation Procedure

1. Install the oil filter.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil pan drain bolt.

Tighten
Tighten the oil pan drain bolt to 26 N·m (19 lb ft).

3. Lower the vehicle.
4. Fill the engine with oil to the appropriate mark.
5. Test the oil level.
6. Start engine and test for leaks.