For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to RUN.
2. Press the washer switch to ON with the wiper switch OFF.

The wipers operate at low speed. The washer sprays the windshield as long as the washer switch is held ON. After releasing the switch, the washer stops and the wipers return to the park position after 3-5 sweeps.

• | Washers Inoperative .

• | Wipers Mist, Delay, and Low Modes Inoperative .

2 | Turn the wiper switch to DELAY (pulse mode). | The wipers make one complete sweep, then pause for 1-22 seconds before making the next sweep. The pause time is adjusted by turning the wiper switch through the delay range. | Wipers Delay Mode Inoperative .
3 |

1. Turn the wiper switch to DELAY.
2. Press the washer switch ON.

The washer sprays the windshield as long as the washer switch is held ON. The wipers run at low speed while spraying and continue for 3-5 sweeps after the washer switch is released. The wipers then return to pulse operation.

• | Washers Inoperative .

• | Wipers Delay Mode Inoperative .

4 | Turn the wiper switch to LO. | The wipers run continuously at low speed. |

• | Wipers Mist, Delay, and Low Modes Inoperative .

• | Wipers All Modes Inoperative .

5 | Turn the wiper switch to HI. | The wipers run continuously at a faster speed. |

• | Wipers High Mode Inoperative, Low Mode Operates .

• | Wipers All Modes Inoperative .

6 | Turn the wipers OFF. | The wipers return to the park position at low speed. | Wipers Blades Do Not Park .
7 | Turn the wiper switch to MIST, then release. | The wipers make one complete sweep, then return to park position. | Wipers Mist, Delay, and Low Modes Inoperative .