For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the transmission with a jack and wood block.
3. Remove the through-bolt.
4. Remove the rear mount to transmission bolts.
5. Remove the rear mount.
6. Remove the 2 rear bracket cradle nuts.
7. Remove the rear bracket to cradle bolt.
8. Remove the bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear bracket and rear bracket to cradle bolt.

Tighten
Tighten the rear bracket to cradle bolt to 66 N·m (49 lb ft).

2. Install the 2 rear bracket to cradle nuts.

Tighten
Tighten the cradle nuts to 66 N·m (49 lb ft).

3. Install the rear mount and the rear mount to transmission bolts.

Tighten
Tighten the rear mount to transmission bolts to 110 N·m (81 lb ft).

4. Install the through-bolt.

Tighten
Tighten the through-bolt to 130 N·m (96 lb ft).

5. Remove the block of wood and jack from underneath the transmission.
6. Lower the vehicle.