For 1990-2009 cars

### Removal Procedure

1. Remove the split/folding rear seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .
2. Untie the drawstrings from the cover.
3. Remove the hog ring retainers.
4. Remove the cover from the pad.

### Installation Procedure

1. Install the cover onto the pad.
2. Pull and tie the drawstrings around the cover.
3. Install the hog ring retainers.
4. Install the split/folding rear seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .