For 1990-2009 cars

### Removal Procedure

1. Remove the HVAC module assembly. Refer to HVAC Module Assembly Replacement .
2. Remove the violet vacuum hose from the vacuum tank.
3. Remove the vacuum tank screw.
4. Remove the vacuum tank from the HVAC module assembly.

Slide the mounting tab from the bracket.

### Installation Procedure

1. Install the vacuum tank to the HVAC module assembly.

Slide the mounting tab into the bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the vacuum tank screw.

Tighten
Tighten the screw to 2 N·m (18 lb in).

3. Connect the violet vacuum tank hose.
4. Install the HVAC module assembly. Refer to HVAC Module Assembly Replacement .