For 1990-2009 cars

### Removal Procedure

1. Adjust the front bucket seat to the full up position in order to gain access to the power seat switch.
2. Pull the bezel from the power seat switch.
3. Adjust the front seat cushion cover in order to gain access to the power seat switch. Refer to Front Seat Cushion Cover Replacement .
4. Remove the power seat switch screws.
5. Disconnect the electrical connector from the power seat switch.
6. Remove the power seat switch from the seat cushion frame.

### Installation Procedure

1. Connect the electrical connector to the power seat switch.
2. Position the power seat switch to the seat cushion frame.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the power seat switch screws.

Tighten
Tighten the screws to 3 N·m (27 lb in).

4. Adjust the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
5. Align the bezel to the power seat switch and press into place until fully seated.
6. Adjust the front bucket seat to the original position.