For 1990-2009 cars

### Removal Procedure

Important: Service the clutch pedal and bracket as an assembly.

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls-2.4L.
2. Remove the sound insulator from inside the vehicle. Refer to Instrument Panel Insulator Panel Replacement - Right Side or the Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.
3. Remove the clutch master cylinder pushrod from the clutch pedal.
4. Disconnect the clutch position switch.
5. Remove the clutch cruise control switch from the bracket.
6. Remove the instrument panel support beam.
7. Remove the instrument panel support beam bracket bolt.
8. Disconnect the cruise control switch.
9. Remove the clutch pedal and bracket mounting nuts.
10. Remove the clutch pedal and bracket assembly.

### Installation Procedure

1. Install the clutch pedal and bracket assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the clutch pedal and bracket mounting nuts.

Tighten
Start with the lower nuts, tighten the nuts to 23 N·m (17 lb ft).

3. Install the instrument support bracket bolt.
4. Install the instrument panel support beam.
5. Install the clutch master cylinder pushrod bushing on the pedal. Lubricate the bushing.
6. Install the clutch master cylinder pushrod to the clutch pedal.
7. Install the cruise control switch.
8. Connect the cruise control switch.
9. Connect the clutch position switch.
10. Adjust the cruise control clutch switch, if equipped. Refer to Cruise Control Cable Adjustment in Cruise Control.
11. Install the sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side or the Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.